<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="1.905" y1="12.065" x2="49.53" y2="12.065" width="0.254" layer="20"/>
<wire x1="49.53" y1="12.065" x2="49.53" y2="4.695" width="0.254" layer="20"/>
<wire x1="49.53" y1="4.695" x2="1.905" y2="4.695" width="0.254" layer="20"/>
<wire x1="1.905" y1="4.695" x2="1.905" y2="12.065" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="Measurement-Specialties">
<description>&lt;B&gt;Measurement Specialties Inc. Devices&lt;/b&gt;&lt;p&gt;
&lt;B&gt; Variometer Module, with stainless steel cap&lt;/b&gt;&lt;p&gt;
&lt;B&gt; MS5611-01BA03&lt;/b&gt;&lt;p&gt;
http://www.meas-spec.com&lt;p&gt;
&lt;author&gt;Created by  S.Hofmann   mc_sho@gmx.de&lt;/author&gt;</description>
<packages>
<package name="SON125P300X500X100-8N">
<description>SON,1.25mm,pitch;8 pin,3.00mm W X 5.00mm L X 1.00mm H body</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="I2C" library="SparkFun" package="1X04" value="i2c">
<attribute name="NAME"/>
</element>
<element name="IC2" library="Measurement-Specialties" package="SON125P300X500X100-8N" value="MS5611-01BA03">
<attribute name="NAME"/>
</element>
<element name="IC3" library="Measurement-Specialties" package="SON125P300X500X100-8N" value="MS5611-01BA03">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="EIA3216" value="0.1µF">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="I2C" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="3"/>
<contactref element="C6" pad="C"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="I2C" pad="2"/>
<contactref element="C6" pad="A"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="I2C" pad="3"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="SCLK">
<contactref element="I2C" pad="4"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC3" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
